# class CameraWhiteBalanceInfo

    class CameraWhiteBalanceInfo implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Setting of white balance.

##### Class Members:

#### Members

method
getWhiteBalanceMode

###### method getWhiteBalanceMode

    CameraWhiteBalanceMode getWhiteBalanceMode()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get setted White Balance.

##### Return:

CameraWhiteBalanceMode | Return setted White Balance.

method
setWhiteBalanceMode

###### method setWhiteBalanceMode

    void setWhiteBalanceMode(CameraWhiteBalanceMode whiteBalanceMode)

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To set White Balance.

##### Input Parameters:

CameraWhiteBalanceMode whiteBalanceMode | White Balance that needs to be set.

method
getColorTemperature

###### method getColorTemperature

    Integer getColorTemperature()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get setted color temperature. Real color temperature value (K) = value * 100. For example, 50 -> 5000K.

##### Return:

Integer | Return setted color temperature.

method
setColorTemperature

###### method setColorTemperature

    void setColorTemperature(Integer colorTemperature)

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To set color temperatur. Unit: kelvin. The color temperature can only be set when the white balance mode is set to `MANUAL`.

##### Input Parameters:

Integer colorTemperature | Color temperature value to be set in the range of [20, 100]. Real color temperature value (K) = value * 100. For example, 50 -> 5000K.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found