# class SuperResolutionInfo

    class SuperResolutionInfo implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

The status and information of super resolution photo shooting.

##### Class Members:

#### Members

method
getMaxArea

###### method getMaxArea

    DoubleRect4Sides getMaxArea()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the maximum area of super resolution photo shooting. This range is automatically calculated by the camera based on the camera angle.

##### Return:

DoubleRect4Sides | Return the maximum area of super resolution photo shooting. (0,0) is the upper left corner of the video interface, (1,1) is the lower right corner of the video interface.

method
getZoomTotalCount

###### method getZoomTotalCount

    Integer getZoomTotalCount()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the total number of zoom photos that need to be taken for super resolution photo shooting.

##### Return:

Integer | Return the total number of zoom photos that need to be taken for super resolution photo shooting.

method
getCaptureArea

###### method getCaptureArea

    DoubleRect4Sides getCaptureArea()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the currently set area of super resolution photo shooting.

##### Return:

DoubleRect4Sides | Return the currently set area of super resolution photo shooting. (0,0) is the upper left corner of the video interface, (1,1) is the lower right corner of the video interface.

method
getCaptureColumnCount

###### method getCaptureColumnCount

    Integer getCaptureColumnCount()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the row number of super resolution photo shooting.

##### Return:

Integer | Return the row number of super resolution photo shooting.

method
getCaptureRowCount

###### method getCaptureRowCount

    Integer getCaptureRowCount()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the column number of super resolution photo shooting.

##### Return:

Integer | Returns the column number of super resolution photo shooting.

method
getIsStorageOverflow

###### method getIsStorageOverflow

    Boolean getIsStorageOverflow()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get whether the SD Card is full.

##### Return:

Boolean | `true` means that the SD Card is full.

method
getCaptureRemainingTime

###### method getCaptureRemainingTime

    Integer getCaptureRemainingTime()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the remaining time of super resolution photo shooting.

##### Return:

Integer | Return the remaining time of super resolution photo shooting.

method
getProgress

###### method getProgress

    Integer getProgress()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the progress of super resolution photo shooting.

##### Return:

Integer | Return the progress of super resolution photo shooting.

method
getZoomCapturedCount

###### method getZoomCapturedCount

    Integer getZoomCapturedCount()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the number of shots taken by super resolution photo shooting.

##### Return:

Integer | Return the number of shots taken by super resolution photo shooting.

method
getStatus

###### method getStatus

    SuperResolutionState getStatus()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the status of super resolution photo shooting.

##### Return:

SuperResolutionState | Return the status of super resolution photo shooting.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found