# class MultiControlLostControlInfo

    class MultiControlLostControlInfo implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.remotecontroller

##### Description:

This class is used to define the information returned when the device with control right loses connection.

##### Class Members:

method
getType

###### method getType

    MultiControlChannel getType()

Package: | dji.sdk.keyvalue.value.remotecontroller

##### Description:

Return channel type of the device that lost connection. 返回失去连接设备的通道类型。

##### Return:

MultiControlChannel | Return channel type of the device that lost connection.

method
getValue

###### method getValue

    List<MultiControlAuthorityTypeInfo> getValue()

Package: | dji.sdk.keyvalue.value.remotecontroller

##### Description:

Return control type of the device that lost connection.

##### Return:

List<MultiControlAuthorityTypeInfo> | Return control type of the device that lost connection.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found