# class AccessLockerEncryptionStatus

    class AccessLockerEncryptionStatus implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.flightcontroller

##### Description:

Security code encryption status.

##### Class Members:

method
getIsFeatureSupported

###### method getIsFeatureSupported

    Boolean getIsFeatureSupported()

Package: | dji.sdk.keyvalue.value.flightcontroller

##### Description:

Gets whether the storage device supports the security code function.

##### Return:

Boolean | Returns whether the storage device supports the security code function.

method
getIsFeatureEnabled

###### method getIsFeatureEnabled

    Boolean getIsFeatureEnabled()

Package: | dji.sdk.keyvalue.value.flightcontroller

##### Description:

Gets whether the security code function of the storage device is enabled.

##### Return:

Boolean | Returns whether the security code function of the storage device is enabled.

method
getIsFeatureNeedToBeVerified

###### method getIsFeatureNeedToBeVerified

    Boolean getIsFeatureNeedToBeVerified()

Package: | dji.sdk.keyvalue.value.flightcontroller

##### Description:

Gets whether the security code of the storage device needs to be verified.

##### Return:

Boolean | Returns whether the security code of the storage device needs to be verified.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found